**Polymer flanges with polypropylene coat**

1. Application in conformity with **"ORDINANCE No. 2 of March 22, 2005 for the design, construction and operation of water supply systems: for pressurized water supply systems";**
2. **Description – reinforced GFK polymer flange with polypropylene;**
3. **All applicable connection methods – mechanic connection;**
4. **Nominal diameter: DN50; DN80; DN100; DN150;**
5. **Nominal pressure (PN)- PN16;**
6. Anticorrosion coating;
7. High chemical resistance;
8. Maximum exploitation temperature – **80оС;**
9. Maximum tightening torque – **105 N.m;**
10. **In conformity with: ISO/IEC 17067:2014**
11. Standard - **БДС EN1902**.



