**FOX – ball valve made of PE100RC**

1. Application in conformity withПредназначение съгласно **"ORDINANCE No. 2 of March 22, 2005 for the design, construction and operation of water supply systems: for pressurized water supply systems";**
2. **Description – ball valve for butt and electrofusion weld made of PE100RC;**
3. Material used for manufacturing**: virgin** certified by an independent instance, **colored black in advance;**
4. Manufacturing technology – injection molding;
5. **All applicable connection methods – butt and electrofusion weld;**
6. **Material – PE100RC, resistant to crack;**
7. **Color – black;**
8. **Flow passing – full;**
9. Full opening at 90о;
10. Possible operation while partly open;
11. **Nominal diameter: DN20; DN25; DN32; DN 40; DN50; DN63; DN75; DN90, DN110, DN125, DN140, DN160, DN180; DN200; DN225; DN250; DN280; DN315;**
12. **Nominal pressure and Standard Dimension Ratio (SDR) - SDR11;**
13. Standard - **БДС EN12201-4**;



